|  |  |
| --- | --- |
| **Joint Collaborative Team on Video Coding (JCT-VC)**  **of ITU-T SG 16 WP 3 and ISO/IEC JTC 1/SC 29/WG 11**  33rd Meeting: Macao, CN, 6–12 Oct. 2018 | Document: JCTVC-AG0024 |

|  |  |  |  |
| --- | --- | --- | --- |
| *Title:* | **Advanced wavefront-based parallel solution decoding for MV-HEVC** | | |
| *Status:* | Input document to JCT-VC | | |
| *Purpose:* | Proposal | | |
| *Author(s) or Contact(s):* | Wei Liu, Yong Beom Cho Address Department of Electronic Engineering, Konkuk University, Seoul, South Korea | Tel: Email: | +82-10-7661-1108 ybcho@konkuk.ac.kr |
| *Source:* | Konkuk University | | |


\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

# Abstract



This paper presents an advanced Wavefront Parallel Processing method which is proposed to achieve higher intra-frame parallelism.

# Introduction

Our proposed approach is to complete tasks in parallel. In each working thread (WT), only the existing task unit needs to be completed to implement the same parallel mode of the decoded row, similar to WPP. The entropy decoder reconstruction pixel (EDRP) task unit is a CTU, and the loop filter (LF) task unit is several CTUs. In order to improve the in-frame parallelism, the EDRP and LF tasks are performed in a pipeline manner, and the LF is processed similar to the WPP method in parallel. In order to satisfy the data-dependent LF task, the previous row is delayed by one LF unit. The LF task is one LF unit later than the entropy reconstruction (ER) task to balance the complexity of processing the EDRP and LF task units without additional computation and schedule tasks between threads. This method reduces the computational load on the CPU. Another advantage is that, when an ER task has higher complexity because its own CTU block needs to be decoded, the following CTU row is waiting. Hence, the WT can perform LF processing. Because of the similar complexity, the complex CTU block decoding is completed and returned to the thread pool while the LF work is being completed. During this time, the CTU waiting for the ER task can continue with using the WT. This method also effectively improves the parallelism within the frame. Fig. 2 shows the time consumption of each function module of MV-HEVC. We found that the EDRP and LF occupied more than 80% of the time. Our analysis showed that the computational complexities of EDRP and LF are related to a certain relationship. The coefficient β is approximately equal to 4. Fig. 1 shows the LF task unit was set to four CTU blocks. When there are less than four CTUs at the end of each line, it is also an LF task unit. The size of the LF task unit can be freely set by adjusting the value of β.



**Fig. 1** ER, LF task assignment and execution sequence.




**Fig. 2** Profiling results for MV-HEVC.


# Proposed parallel decoding

The proposed parallel method for intra-frame implementation is given in Algorithms 1 and 2. Algorithm 1 generates the MT task queue and wakes up the WT. Algorithm 2 searches the WT and performs the computation work. The FT is responsible for initializing the work, adding the first row of ER tasks to the ER queue, and waking the WT to work. The FT also monitor the computing units that can be queued in the parallel region of each frame. The WT first searches for tasks in the ER queue. If it is the first row, it decompresses the current line. If it is not the first row, after it executes the CTU task of the current row, it returns to the thread pool and waits to be awakened for the task. If the ER queue is empty, then the thread is woken up in the LF queue. This ensures that the ER task has a higher priority than the LF task so that the former is always executed first. This ensures that enough reconstructed CTUs are executed by the LF.

**Table 1** Variables for the pseudo code.

|  |  |
| --- | --- |
|  | Task queue 𝑛 ∈0 1 2 3 (v\_(n ) = 3) |
|  | Entropy decoder & Reconstruction pixel task queue |
|  | Loop Filter task queue |
|  | CTU rows structure |
|  | Completed ER task of CTUs in current row |
|  | Completed LF task of CTUs in current row |
|  | ER working state of current row |
|  | LF working state of current row |
|  | State of ER task pushed into task queue in current row |
|  | State of LF task pushed into task queue in current row |
|  | The number of CTUs with LF unit |
|  | The number of rows with a frame |
|  | The number of CTUs with a Row |
|  | Start row of parallel area |
|  | End row of parallel area |





# Patent rights declaration(s)

**Konkuk University does not have any current or pending patent rights relating to the technology described in this contribution.**