
HM software: Encoder Version [5.0][Windows][VS 1500][32 bit] 

Input          File          : D:\HEVC\InputSequences\classD\BQSquare_416x240_60.yuv
Bitstream      File          : str.bin
Reconstruction File          : rec.yuv
Real     Format              : 416x240 60Hz
Internal Format              : 416x240 60Hz
Frame index                  : 0 - 15 (16 frames)
CU size / depth              : 64 / 4
RQT trans. size (min / max)  : 4 / 32
Max RQT depth inter          : 3
Max RQT depth intra          : 3
Min PCM size                 : 128
Motion search range          : 64
Intra period                 : 32
Decoding refresh type        : 1
QP                           : 32.00
Max dQP signaling depth      : 0
GOP size                     : 8
Internal bit depth           : 8
PCM sample bit depth         : 8
DisableInter4x4              : 1

TOOL CFG: ALF:1 IBD:0 HAD:1 SRD:1 RDQ:1 SQP:0 ASR:0 PAD:0 LComb:1 LCMod:0 FEN:1 ECU:0 CFM:0 RQT:1 MRG:1 LMC:1 Slice: G=0 M=0 EntropySlice: M=0 CIP:0 SAO:1 PCM:0 WPP:0 WPB:0 TileBoundaryIndependence:1 TileLocationInSliceHdr:1 TileMarker:1[4]  WaveFrontSynchro:2 WaveFrontFlush:1 WaveFrontSubstreams:4

Length of substream [0]: 3981 bytes -- 31852 bits
Length of substream [1]: 3692 bytes -- 29532 bits
Length of substream [2]: 2757 bytes -- 22057 bits
Length of substream [3]: 1640 bytes -- 13120 bits
POC    0 TId: 0 ( I-SLICE, QP 32 )      97464 bits [Y 34.0186 dB    U 39.8240 dB    V 40.4523 dB] [ET    16 ] [L0 ] [L1 ] [MD5:6077fe8857b56bb8bb0eeea043d31cec]
Length of substream [0]: 1223 bytes -- 9791 bits
Length of substream [1]: 555 bytes -- 4437 bits
Length of substream [2]: 497 bytes -- 3979 bits
Length of substream [3]: 535 bytes -- 4278 bits
POC    8 TId: 0 ( B-SLICE, QP 33 )      23000 bits [Y 33.0453 dB    U 39.7393 dB    V 40.4045 dB] [ET    39 ] [L0 0 ] [L1 0 ] [LC 0 ] [MD5:743758fca19f6daa22b8b037b2d53fab]
Length of substream [0]: 199 bytes -- 1592 bits
Length of substream [1]: 17 bytes -- 142 bits
Length of substream [2]: 20 bytes -- 156 bits
Length of substream [3]: 124 bytes -- 996 bits
POC    4 TId: 0 ( B-SLICE, QP 34 )       3296 bits [Y 32.3210 dB    U 39.8063 dB    V 40.4507 dB] [ET    34 ] [L0 0 8 ] [L1 8 0 ] [LC 0 8 ] [MD5:4ab9ca6c495fe9478fdcfe9a3ef76e0f]
Length of substream [0]: 52 bytes -- 423 bits
Length of substream [1]: 9 bytes -- 67 bits
Length of substream [2]: 7 bytes -- 60 bits
Length of substream [3]: 32 bytes -- 250 bits
POC    2 TId: 0 ( B-SLICE, QP 35 )       1144 bits [Y 32.6487 dB    U 39.7663 dB    V 40.3985 dB] [ET    31 ] [L0 0 4 ] [L1 4 8 ] [LC 0 4 8 ] [MD5:f5485470b3cdb4f709326aa0f12bce1f]
Length of substream [0]: 8 bytes -- 71 bits
Length of substream [1]: 2 bytes -- 14 bits
Length of substream [2]: 3 bytes -- 20 bits
Length of substream [3]: 7 bytes -- 57 bits
POC    1 TId: 0 ( b-SLICE, QP 36 )        336 bits [Y 33.0263 dB    U 39.7921 dB    V 40.4162 dB] [ET    27 ] [L0 0 2 ] [L1 2 4 ] [LC 0 2 4 ] [MD5:64526fc5e7acae0f4c82cf8328f3059e]
Length of substream [0]: 5 bytes -- 41 bits
Length of substream [1]: 3 bytes -- 25 bits
Length of substream [2]: 3 bytes -- 25 bits
Length of substream [3]: 6 bytes -- 52 bits
POC    3 TId: 0 ( b-SLICE, QP 36 )        312 bits [Y 32.3397 dB    U 39.7832 dB    V 40.4052 dB] [ET    26 ] [L0 2 0 ] [L1 4 8 ] [LC 2 4 0 8 ] [MD5:9d23aa63f67798585e35f0a400223412]
Length of substream [0]: 73 bytes -- 587 bits
Length of substream [1]: 2 bytes -- 20 bits
Length of substream [2]: 7 bytes -- 52 bits
Length of substream [3]: 32 bytes -- 259 bits
POC    6 TId: 0 ( B-SLICE, QP 35 )       1296 bits [Y 32.3842 dB    U 39.8357 dB    V 40.4374 dB] [ET    23 ] [L0 4 2 ] [L1 8 4 ] [LC 4 8 2 ] [MD5:2552508b033f9cdda519449b33fd58a8]
Length of substream [0]: 9 bytes -- 78 bits
Length of substream [1]: 2 bytes -- 15 bits
Length of substream [2]: 5 bytes -- 35 bits
Length of substream [3]: 4 bytes -- 36 bits
POC    5 TId: 0 ( b-SLICE, QP 36 )        336 bits [Y 32.2334 dB    U 39.7790 dB    V 40.3754 dB] [ET    23 ] [L0 4 0 ] [L1 6 8 ] [LC 4 6 0 8 ] [MD5:68a15d0c81143b220737f4b498ce1f45]
Length of substream [0]: 16 bytes -- 134 bits
Length of substream [1]: 2 bytes -- 14 bits
Length of substream [2]: 3 bytes -- 20 bits
Length of substream [3]: 5 bytes -- 46 bits
POC    7 TId: 0 ( b-SLICE, QP 36 )        384 bits [Y 32.5877 dB    U 39.7798 dB    V 40.3985 dB] [ET    21 ] [L0 6 4 ] [L1 8 6 ] [LC 6 8 4 ] [MD5:01b726cc1378237501dad5f853fcacb9]
Length of substream [0]: 405 bytes -- 3246 bits
Length of substream [1]: 67 bytes -- 530 bits
Length of substream [2]: 59 bytes -- 473 bits
Length of substream [3]: 162 bytes -- 1295 bits
POC   12 TId: 0 ( B-SLICE, QP 34 )       6128 bits [Y 31.4583 dB    U 39.6652 dB    V 40.2300 dB] [ET    30 ] [L0 8 6 ] [L1 8 6 ] [LC 8 6 ] [MD5:151f0ae028f99c558b5cb4a2f51644be]
Length of substream [0]: 76 bytes -- 610 bits
Length of substream [1]: 2 bytes -- 20 bits
Length of substream [2]: 8 bytes -- 58 bits
Length of substream [3]: 36 bytes -- 293 bits
POC   10 TId: 0 ( B-SLICE, QP 35 )       1280 bits [Y 31.9599 dB    U 39.7102 dB    V 40.3292 dB] [ET    27 ] [L0 8 6 ] [L1 12 8 ] [LC 8 12 6 ] [MD5:3a96e01209e3296720adea861ab37fe9]
Length of substream [0]: 11 bytes -- 88 bits
Length of substream [1]: 2 bytes -- 16 bits
Length of substream [2]: 3 bytes -- 30 bits
Length of substream [3]: 5 bytes -- 35 bits
POC    9 TId: 0 ( b-SLICE, QP 36 )        360 bits [Y 32.3990 dB    U 39.7131 dB    V 40.3575 dB] [ET    26 ] [L0 8 10 ] [L1 10 12 ] [LC 8 10 12 ] [MD5:b113c11febf7bbdaac4da4c68f3bda21]
Length of substream [0]: 13 bytes -- 108 bits
Length of substream [1]: 2 bytes -- 16 bits
Length of substream [2]: 4 bytes -- 30 bits
Length of substream [3]: 4 bytes -- 31 bits
POC   11 TId: 0 ( b-SLICE, QP 36 )        416 bits [Y 31.6004 dB    U 39.6984 dB    V 40.3100 dB] [ET    23 ] [L0 10 8 ] [L1 12 10 ] [LC 10 12 8 ] [MD5:b1d1cab60c6c127d43eddadc4b4c95f9]
Length of substream [0]: 188 bytes -- 1511 bits
Length of substream [1]: 34 bytes -- 270 bits
Length of substream [2]: 32 bytes -- 251 bits
Length of substream [3]: 96 bytes -- 769 bits
POC   14 TId: 0 ( B-SLICE, QP 35 )       3096 bits [Y 30.9106 dB    U 39.6157 dB    V 40.1520 dB] [ET    25 ] [L0 12 10 ] [L1 12 10 ] [LC 12 10 ] [MD5:0b6c187255f12566d955d5d316b0f3e0]
Length of substream [0]: 12 bytes -- 103 bits
Length of substream [1]: 3 bytes -- 23 bits
Length of substream [2]: 5 bytes -- 34 bits
Length of substream [3]: 3 bytes -- 30 bits
POC   13 TId: 0 ( b-SLICE, QP 36 )        368 bits [Y 31.2841 dB    U 39.6101 dB    V 40.2344 dB] [ET    21 ] [L0 12 8 ] [L1 14 12 ] [LC 12 14 8 ] [MD5:2f4927a0e1698b1ceaa3cf6bb53874d0]
Length of substream [0]: 53 bytes -- 424 bits
Length of substream [1]: 4 bytes -- 36 bits
Length of substream [2]: 6 bytes -- 51 bits
Length of substream [3]: 21 bytes -- 162 bits
POC   15 TId: 0 ( b-SLICE, QP 36 )        912 bits [Y 30.1932 dB    U 39.5647 dB    V 40.1350 dB] [ET    20 ] [L0 14 12 ] [L1 14 12 ] [LC 14 12 ] [MD5:703ca6e824c48c52ff204f7f508bea29]


SUMMARY --------------------------------------------------------
	Total Frames |  Bitrate    Y-PSNR    U-PSNR    V-PSNR 
	       16    a    525.4800   32.1507   39.7302   40.3429


I Slices--------------------------------------------------------
	Total Frames |  Bitrate    Y-PSNR    U-PSNR    V-PSNR 
	        1    i   5847.8400   34.0186   39.8240   40.4523


P Slices--------------------------------------------------------
	Total Frames |  Bitrate    Y-PSNR    U-PSNR    V-PSNR 
	        0    p     -1.#IND   -1.#IND   -1.#IND   -1.#IND


B Slices--------------------------------------------------------
	Total Frames |  Bitrate    Y-PSNR    U-PSNR    V-PSNR 
	       15    b    170.6560   32.0261   39.7239   40.3356

RVM: 0.000
Bytes written to file: 18035 (541.050 kbps)

 Total Time:      413.464 sec.
