|  |  |
| --- | --- |
| **Joint Collaborative Team on Video Coding (JCT-VC)**  **of ITU-T SG 16 WP 3 and ISO/IEC JTC 1/SC 29/WG 11**  10th Meeting: Stockholm, SE, 11–20 July 2012 | Document: JCTVC-J0463 |

|  |  |  |  |
| --- | --- | --- | --- |
| *Title:* | **Mental cross-check of JCTVC-J0229** | | |
| *Status:* | Input Document to JCT-VC | | |
| *Purpose:* | Information | | |
| *Author(s) or Contact(s):* | Ye-Kui Wang  5775 Morehouse Drive, San Diego, CA 92121-1714 USA | Tel: Email: | 1-858-651-8345 [yekuiw@qualcomm.com](mailto:yekuiw@qualcomm.com) |
| *Source:* | Qualcomm Incorporated | | |

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

# Abstract

This document provides a mental cross-check for JCTVC-J0229.

It is claimed that the authors of this document understand what is being proposed in JCTVC-J0229. The authors of this document would like to summarize the proposal in JCTVC-J0229, which includes four proposal pieces, as follows.

1. Add the definition sequence start point (SSP) access unit and SSP picture - this is an editorial proposal
2. Add two RPS related constraints, one for RAP pictures, and one for TFD pictures
3. Remove the decoding process for generating unavailable reference pictures in subclause 8.3.3 unless the need is justified
4. Change the TFD picture definition, not to state if a TFD picture can or cannot be correctly decodable but just to state that it is not decoded and not output. It is also suggested to use RAS (random access skip) instead of TFD (tagged for discard)

# Patent rights declaration(s)

**Qualcomm Incorporated does not have current or pending patent rights relating to the technology described in this contribution.**