|  |  |
| --- | --- |
| **Joint Collaborative Team on Video Coding (JCT-VC)**  **of ITU-T SG 16 WP 3 and ISO/IEC JTC 1/SC 29/WG 11**  12th Meeting: Geneva, CH, 14–23 Jan. 2013 | Document: JCTVC-L0380 |

|  |  |  |  |
| --- | --- | --- | --- |
| *Title:* | **AhG4: Subjective evaluation of HEVC intra coding for still image compression** | | |
| *Status:* | Input Document | | |
| *Purpose:* | Information | | |
| *Author(s) or Contact(s):* | Philippe Hanhart Martin Rerabek Pavel Korshunov Touradj Ebrahimi | Email: | philippe.hanhart@epfl.ch |
| *Source:* | Ecole Polytechnique Fédérale de Lausanne (EPFL) | | |

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

# Abstract

This contribution provides a detailed analysis and performance comparison of HEVC intra coding with JPEG and JPEG 2000 (both 4:2:0 and 4:4:4 configurations) for still image compression via a series of subjective and objective evaluations. The evaluation results demonstrate that HEVC intra coding outperforms standard codecs for still images with the average bit rate reduction ranging from 16% (compared to JPEG 2000 4:4:4) up to 43% (compared to JPEG).

# Introduction

As a future video compression standard, HEVC is demonstrating significant quality gains when compared to state of the art video codecs, such as H.264/MPEG-4 AVC. Such effectiveness in video compression suggests the potential efficiency of using HEVC intra coding for still images. This possibility is investigated in a few studies that compare still images compression standards with HEVC intra coding by using PSNR as an objective metric for visual quality (JCTVC-I0595, JCTVC-I0461). Such objective evaluations demonstrate that HEVC can achieve a considerable gain even compared to the state of the art JPEG 2000 compression standard. However, the PSNR metric, despite its popularity in visual quality evaluations, does not accurately reflect perceptual visual quality of human visual system (Sheikh *et al.*, 2006). In addition, the lack of standardization in the field of objective quality assessment and the lack of extensive and commonly accepted comparisons of the different metrics make the PSNR-based assessments rather questionable. Therefore, to fully confirm the claim raised by objective evaluations on the effectiveness of HEVC intra coding for still images, a formal subjective evaluation is necessary.

This contribution performs both objective and subjective evaluations (with emphasis on subjective methodology) of HEVC intra coding for still image compression following the guidelines defined by the JPEG committee for the evaluation of JPEG XR (De Simone *et al.*, 2009). HEVC intra coding is compared to the existing JPEG and JPEG 2000 (both 4:2:0 and 4:4:4 configurations are used) standards using high resolution  bpp images. The compression efficiency is evaluated by means of PSNR objective metric, for comparison with previous work, and subjective tests, which have been conducted in a specific testing environment and following formal evaluation methodology recommended by ITU-R (ITU-R BT.500-13).

This contribution describes the evaluation environment, dataset used, and encoding algorithms in Section 2, and detailed evaluation methodology in Section 3. Subjective and objective results comparing HEVC intra coding with JPEG and JPEG 2000 algorithms are presented and discussed in Section 5. The contribution is concluded in Section 6.

# Test environment

The experiments were conducted at the MMSPG quality test laboratory, which fulfills the recommendations for the subjective evaluation of visual data issued by ITU-R (ITU-R BT.500-13), and was also used by the JPEG committee in the assessment of JPEG XR standard during its development. The laboratory setup was intended to ensure the reproducibility of the subjective tests results by avoiding unintended influence of external factors. The test area was controlled by an indoor video security system to keep track of all the test activities and possible unexpected events, which could affect the test results.

An Eizo CG301W LCD monitor with a native resolution of  pixels was used to display the test stimuli. The monitor was calibrated using an EyeOne Display2 color calibration device according to the following profile: sRGB Gamut, D65 white point, 120 cd/m brightness, and minimum black level. The room was further equipped with a controlled lighting system that consists of neon lamps with 6500 K color temperature, while the color of all the background walls and curtains present in the test area were in mid grey. The illumination level measured on the screen was 15 lux and the ambient black level was 0.2 cd/m.

The experiment involved only one subject per display assessing the test materials. Subjects were seated in line with the center of the monitor, at a distance approximately equal to the height of the screen, but were encouraged to vary the viewing distance whenever needed, to inspect the high resolution image shown on the screen.

# Dataset

The dataset from the JPEG XR evaluation[[1]](#footnote-1) was used in this study. All the images had a resolution of  pixels and were available in RGB 4:4:4 uncompressed format. The whole image set was split into a training set of  images (referred to as *p04*, *p14*, *p22*, and *p30*) and a testing set of  images (referred to as *p01*, *p06*, *p10*, *bike*, *cafe*, and *woman*). Figure 1 provides an overview of the dataset. This set of images was coded using the  codecs and  different coding configurations described below. Similarly to the JPEG XR evaluation (De Simone *et al.*, 2009), the following bit rates were selected: , , , ,  and  bpp. Thus, this resulted in a final test set of  coded images used for the subjective evaluation.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
|  | PhD:Publications:VPQM2013_HEVC:images:p04_small.png | PhD:Publications:VPQM2013_HEVC:images:p14_small.png | PhD:Publications:VPQM2013_HEVC:images:p22_small.png | PhD:Publications:VPQM2013_HEVC:images:p30_small.png |  |
|  | (a) p04 | (b) p14 | (c) p22 | (d) p30 |  |
| PhD:Publications:VPQM2013_HEVC:images:p01_small.png | PhD:Publications:VPQM2013_HEVC:images:p06_small.png | PhD:Publications:VPQM2013_HEVC:images:p10_small.png | PhD:Publications:VPQM2013_HEVC:images:bike_small.png | PhD:Publications:VPQM2013_HEVC:images:cafe_small.png | PhD:Publications:VPQM2013_HEVC:images:woman_small.png |
| (e) p01 | (f) p06 | (g) p10 | (h) bike | (i) cafe | (j) woman |

*Figure 1 – Dataset: training set (a-d) and testing set (e-j).*

The JPEG compressed images were produced using the IJG implementation[[2]](#footnote-2), version 6b. The images were coded in Baseline Profile and the target coding bit rates were controlled by varying the *quality factor* input parameter.

For JPEG 2000 coding, the Kakadu implementation[[3]](#footnote-3) version 6.0 was used. Two different configurations were considered. The first configuration uses chrominance subsampling, which requires external pre- and post-processing steps. Since the weighting tables in JPEG 2000 have been designed and optimized for 4:4:4 content, visual weighting was disabled in this configuration. The following parameters were used:

* Pre-processing: RGB to YCbCr conversion and 4:4:4 to 4:2:0 downsampling.
*  code block size, 1 layer, no precincts,  wavelets, and 5 decomposition levels.
* No visual weighting.
* Post-processing: 4:2:0 to 4:4:4 upsampling and YCbCr to RGB color conversion.

As visual weighting impacts the performance of the JPEG 2000 codec, a second configuration with visual weighting enabled was also included in the evaluations. The parameters in this second configuration were the same as before but the pre- and post-processing steps were discarded and the RGB 4:4:4 images were encoded directly without any subsampling. The *rate control* option was used to encode the images at the target coding bit rates.

In this study, the HEVC Test Model[[4]](#footnote-4), version 8.0rc2, was used. As for JPEG 2000, the images were converted from RGB 4:4:4 to YCbCr 4:2:0 prior to encoding and then back-converted to obtain the final decoded image. The images were coded in Main Intra Profile and the target bit rates were obtained by varying the *quantization parameter*.

# Test methodology

The subjective quality evaluations to compare the image compression algorithms described in Section 3 were conducted following the methodology proposed in (De Simone *et al.*, 2009). As an adaptation of the double-stimulus continuous quality scale (DSCQS) method for video quality evaluation (ITU-R BT.500-13), the selected method implies that two images are displayed simultaneously by splitting the screen horizontally into two parts. One of the two images was always the reference (unimpaired) image. The other was the test image, which in this study was a compressed version of the reference. The position of the reference image on the screen was randomly selected at each visualization. Instead of judging the quality of both images, the subject was asked to detect the impaired image in the pair and rate its quality, using a continuous quality scale ranging from  to , associated with  distinct quality levels (*Bad, Poor, Fair, Good, and Excellent*).

## Training session

Before the test starts, oral instructions were provided to the subject to explain his/her task. Additionally, a training session was organized to allow subjects to familiarize with the assessment procedure and the graphical user interface. The contents shown in the training session were not used in the test session and the data gathered during the training were not included in the final test results. The 4 training contents, shown in Figure 1, were coded with the different codecs and bit rates described in Section 3. Five training samples were manually selected by expert viewers so that the quality of samples were representative of all categorical quality levels on the rating scale. The training materials were presented to subjects exactly as for the test materials, thus in side by side image pairs, where one of the two stimuli was always the unimpaired image.

## Test session

Since the total number of test samples was too large for a single test session, the overall experiment was split into  sessions of approximatively  minutes each. After each session, each subject took a  minutes break before starting the next session. Each session included test materials corresponding to  contents (*p01*, *p06*, *p10* in sessions  and  and *bike*, *cafe*, *woman* in sessions  and ), all the codecs under analysis, and only a subset of the bit rates, which were uniformly distributed across all the sessions.

Four dummy pairs, whose scores were not included in the results, were included at the beginning of each session to stabilize the subjects' ratings. To reduce contextual effects, the stimuli orders of display were randomized applying different permutation for each subject, while the same content was never shown consecutively.

A total of  subjects,  female and  male, took part in the test, completing all the test sessions. All participants were screened for correct visual acuity and color vision using Snellen and Ishiara charts, respectively.

## Analysis of the results

After collecting the scores from the individual subjects, the following statistical tools were applied to analyze the preferences for the different content, compression algorithms, and bit rates.

### Outlier detection

To detect and remove subjects whose scores appear to deviate strongly from others in a session, outlier detection was performed. The outlier detection was applied to the set of results obtained from the  subjects and performed according to the guidelines described in Section 2.3.1 of Annex 2 of (ITU-R BT.500-13). In this study,  outliers were detected in session  and  outlier was detected in session .

### Mean opinion scores and confidence intervals

Statistical measures were computed to describe the score distribution across the subjects for each of the test conditions (combination of content, codec, and bit rate). The mean opinion score (MOS) was computed as:



where  is the number of valid subjects and  is the score by subject  for the test condition .

The relationship between the estimated mean values based on a sample of the population (i.e., the subjects who took part in our experiments) and the true mean values of the entire population is given by the confidence interval of the estimated mean. The  confidence intervals (CI) for MOSs were computed using the Student's *t*-distribution, as follows:



where  is the -value corresponding to a two-tailed Student's *t*-distribution with  degrees of freedom and a desired significance level  (equal to 1-degree of confidence).  corresponds to the number of valid subjects, and  is the standard deviation of a single test condition  across the subjects . The confidence intervals were computed for an  equal to , which corresponds to a degree of significance of .

### Relationship between estimated mean values

To understand whether the difference between two MOS values corresponding to two different codecs is statistically significant, a multiple comparison significance procedure was applied to the data (Snedecor and Cochran, 1989). Particularly, for each bit rate and content, a one-way ANOVA test was conducted to compare all the codecs pairwise to understand whether the differences of their means were statistically significant (Snedecor and Cochran, 1989).

### Bit rate reduction

To evaluate the coding efficiency of HEVC intra coding, the Bjøntegaard model (Bjøntegaard, 2008) and PSNR values were used to determine the objective bit rate reduction . Similarly, using MOS values instead of PSNR values, the subjective bit rate reduction, , was estimated.  is more realistic since it is based on perceived quality, while  is based on estimated quality.  was computed using a third order logarithmic polynomial fitting of the data points, as proposed in (Bjøntegaard, 2008).  was computed using finite integration and piecewise linear interpolation on the monotonic part of the subjective rate-distortion curves.

# Results and discussion

The PSNR based rate-distortion performance for all compression algorithms and contents is shown in Figure 2. It is clear that HEVC outperforms other codecs across the majority of contents and through most investigated bit rates. JPEG 2000 with 4:2:0 sampling configuration is the only competitive compression algorithm in comparison to HEVC, especially for content *p01*. The observed performance difference of JPEG 2000 4:2:0 and HEVC in terms of PSNR is between  -  dB for all tested bit rates and contents. Furthermore, the PSNR improvement of HEVC relative to JPEG 2000 4:4:4 and JPEG varies through all tested contents and bit rates between  -  dB and  -  dB, respectively.

Similar results for still image compression performance comparison based on objective metrics have been reported in two recent studies. Using the dataset containing, among others, the images described in Section 3, HEVC HM 6.0 encoder and reference software encoders for other standards, Nguyen and Marpe (JCTVC-I0595) have reported an average bit rate reduction of  and  for HEVC intra coding over JPEG and JPEG 2000 4:2:0, respectively. Additionally, Lainema and Ugur (JCTVC-I0461) have reported an average bit rate reduction of  over JPEG. The  values reported in Table 1 are similar to those reported in above mentioned studies and confirm that, according to objective evaluations based on PSNR, a significant bit rate reduction can be achieved for HEVC intra coding over the JPEG standards.

The subjective rate-distortion plots illustrating the MOS and CI values for each content are shown in Figure 3. For each content, the MOS values span the entire range of quality levels. The only exception to this overall behaviour is on content *cafe*, whose structure is sensitive to compression artifacts and therefore, even for the highest bit rate, the image quality is rated below .

An overall impression of the performance of the different codecs can be obtained when looking closely at the rate-distortion plots in Figure 3. In general, all examined coding standards have the same or very similar performance at the highest bit rate. However, at lower bit rates, the performance of individual coding algorithms varies significantly depending on the content. While HEVC outperforms (particularly at bit rates below  bpp) other coding algorithms for contents *bike*, *cafe*, and *p10*, its performance is quite comparable to both versions of JPEG 2000 for contents *p01* and *p06*. Moreover, HEVC shows always better or equal performance than JPEG with the exception of content *woman*. Looking at the MOS results of the image *woman*, which consists in a woman's face portrait, one can see that HEVC is outperformed by JPEG and JPEG 2000 4:4:4. While JPEG outperforms HEVC only at  bpp and  bpp, JPEG 2000 4:4:4 seems to be better for all bit rates below  bpp ( bpp included). This might be explained by the specific banding artifacts introduced by HEVC at lower bit rates for this particular content. Such banding artifacts are subjectively more disturbing in comparison to the typical blurring effect introduced by JPEG 2000 4:4:4 coding.

The estimated bit rate saving based on MOS for HEVC relative to JPEG, JPEG 2000 4:2:0, and JPEG 2000 4:4:4 is about , , and , respectively. The differences between  and  values (see Table 1) show the importance of subjective tests to determine a more realistic estimation of the achievable bit rate reduction .

Interesting observations can be made by looking at the mutual comparison of both versions of JPEG 2000. Although JPEG 2000 4:2:0 performs always better than JPEG 2000 4:4:4 in terms of PSNR, the subjective results dictate the opposite. This might be explained by the fact that visual weighting was disabled for JPEG 2000 4:2:0 while it was enabled for the second color sampling configuration of JPEG 2000. The lack of the visual weighting creates strong distortions, especially on the skin texture at lower bit rates, as reported during development of JPEG 2000 standard, which is not captured by PSNR based metric.

The results of the multiple comparison test, detecting the significant difference pairwise among individual codecs and comparing the performance of HEVC to all other codecs for all test conditions, are presented in Table 2. These results confirm all the findings from the rate distortion plots. While at the highest bit rate, all compression standards perform equally, at bit rates lower than  bpp, HEVC performs usually better, or at least equal, when compared to all other standards, except for JPEG 2000 4:4:4 on content *woman*. JPEG 2000 4:4:4 is the second best performing compression algorithm while its performance is the same as for HEVC in  out of  cases. On the other hand, JPEG performs practically always worse than HEVC.

Table 1: Overall bit rate reduction for HEVC relative to all examined standards as an anchor.

|  |  |  |  |
| --- | --- | --- | --- |
|  | **Codec** | | |
| **Metric** | **JPEG** | **JPEG 2000 4:2:0** | **JPEG 2000 4:4:4** |
|  | -61.63% | -20.26% | -46.88% |
|  | -43.10% | -30.96% | -15.98% |

Table 2: Results of the multiple comparison test expressed in terms of number of contents for which HEVC performs better, equal, or worse than the other codecs.

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
|  | **Bit rate [bpp]** | | | | | |
| **Condition** | **0.25** | **0.50** | **0.75** | **1.00** | **1.25** | **1.50** |
| HEVC > JPEG | 6 | 6 | 5 | 1 | 3 | 0 |
| HEVC = JPEG | 0 | 0 | 1 | 4 | 3 | 6 |
| HEVC < JPEG | 0 | 0 | 0 | 1 | 0 | 0 |
| HEVC > JPEG 2000 4:2:0 | 4 | 3 | 5 | 1 | 4 | 0 |
| HEVC = JPEG 2000 4:2:0 | 2 | 3 | 1 | 5 | 2 | 6 |
| HEVC < JPEG 2000 4:2:0 | 0 | 0 | 0 | 0 | 0 | 0 |
| HEVC > JPEG 2000 4:4:4 | 3 | 3 | 4 | 1 | 1 | 0 |
| HEVC = JPEG 2000 4:4:4 | 2 | 2 | 1 | 4 | 5 | 6 |
| HEVC < JPEG 2000 4:4:4 | 1 | 1 | 1 | 1 | 0 | 0 |

|  |  |
| --- | --- |
|  |  |
|  |  |
|  |  |

*Figure 2 – Rate-distortion performance.*

|  |  |
| --- | --- |
|  |  |
|  |  |
|  |  |

*Figure 3 – Mean opinion scores vs. bit rate for the different compression algorithm across the test images.*

# Conclusion

In this contribution, the subjective quality assessment of HEVC intra coding for still image compression is described in details. The upcoming video compression standard HEVC has been compared to existing and well established compression algorithms JPEG and JPEG 2000. The subjective evaluations were conducted according the guidelines defined by the JPEG committee for the evaluation of JPEG XR. The obtained results, including detailed statistical analysis allowing the accurate comparison of the various codecs performance, are presented and discussed in details.

The evaluation results demonstrate that HEVC intra coding outperforms encoders for still images with an average bit rate reduction ranging from  (compared to JPEG 2000 4:4:4) up to  (compared to JPEG).

# References

G. Bjøntegaard. “Improvements of the BD-PSNR model,” ITU-T SG16/Q6, Doc. VCEG-AI11, 35th VCEG Meeting, Berlin, Germany, July 2008.

F. De Simone, L. Goldmann, V. Baroncini, and T. Ebrahimi, “Subjective evaluation of JPEG XR image compression,” in Proceedings of SPIE, Applications of Digital Image Processing XXXII, August 2009.

ITU-R, Recommendation ITU-R BT.500-13.

J. Lainema and K. Ugur, “On HEVC still picture coding performance,” Doc. JCTVC-I0461, Geneva, Switzerland, April-May 2012.

T. Nguyen and D. Marpe, “Performance Comparison of HM 6.0 with Existing Still Image Compression Schemes Using a Test Set of Popular Still Images,” Doc. JCTVC-I0595, Geneva, Switzerland, April-May 2012.

H.R. Sheikh, M.F. Sabir, and A.C. Bovik, “A Statistical Evaluation of Recent Full Reference Image Quality Assessment Algorithms,” in IEEE Transactions on Image Processing, vol. 15, no. 11, pp. 3440-3451, November 2006.

G. W. Snedecor and W. G. Cochran, *Statistical Methods,* Iowa State University Press, 1989.

# Patent rights declaration(s)

**EPFL does not have any current or pending patent rights relating to the technology described in this contribution.**

1. http://mmspg.epfl.ch/iqa [↑](#footnote-ref-1)
2. http://www.ijg.org/ [↑](#footnote-ref-2)
3. http://www.kakadusoftware.com/ [↑](#footnote-ref-3)
4. https://hevc.hhi.fraunhofer.de/ [↑](#footnote-ref-4)