|  |  |
| --- | --- |
| **Joint Collaborative Team on Video Coding (JCT-VC)**  **of ITU-T SG 16 WP 3 and ISO/IEC JTC 1/SC 29/WG 11**  13th Meeting: Incheon, KR, 18–26 Apr. 2013 | Document: JCTVC-M0331 |

|  |  |  |  |
| --- | --- | --- | --- |
| *Title:* | **SCE1: Results of Test 4.2.2 and 4.2.3 on Difference Intra prediction** | | |
| *Status:* | Input Document to JCT-VC | | |
| *Purpose:* | Proposal | | |
| *Author(s) or Contact(s):* | Krishna Rapaka  Jianle Chen  Xiang Li  Marta Karczewicz | Tel: Email: | [krapaka@qti.qualcomm.com](mailto:krapaka@qti.qualcomm.com)  [cjianle@qti.qualcomm.com](mailto:cjianle@qti.qualcomm.com)  [lxiang@qti.qualcomm.com](mailto:lxiang@qti.qualcomm.com)  [martak@qti.qualcomm.com](mailto:martak@qti.qualcomm.com) |
| *Source:* | Qualcomm Incorporated | | |

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

# Abstract

This document reports SHVC SCE1 results of test 4.2.2 and 4.2.3 on Difference domain Intra Prediction (DIP). DIP is a predictive coding tool which uses reconstructed pixels from spatial neighbors of current enhancement layer and co-located base layer to predict the current enhancement layer block. It is reported that an average of 0.7% (EL+BL), luma BD-rate reduction is obtained for AI Spatial scalability cases.

# Technical description

This test studies the Difference domain Intra Prediction (DIP) proposed in [1][2] to improve the coding efficiency of SHVC. In the DIP, as shown in Figure 1, the difference between the pixels of current neighbors and those of collocated BL neighbors are used to generate a difference prediction based on the intra prediction mode. The generated difference prediction signal is added to the collocated BL block signal to form the final prediction.

Due to the high frequency nature of the difference signals, HEVC mode dependent intra smoothing (MDIS) process and intra filtering for horizontal, vertical and DC mode are disabled in difference domain intra prediction. As a result, the latency and complexity are reduced without loss in BD-Rate.

The difference domain Prediction mode is indicated by a flag *intra\_resi\_pred\_flag* at CU level.



Figure 1 Intra residual prediction

# Test Results

The proposed method is implemented on SHM-1.0 intraBL framework and experimentally verified under SHVC common test conditions defined by JCTVC-L1009 and the results are summarized in the following tables for AI 2x and 1.5x spatial scalability cases. Thanks to LG Electronics for crosschecking the tests.

**Table 1: Experimental results of Difference Domain Intra Prediction for AI configuration**

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
|  | **AI HEVC 2x** | | | **AI HEVC 1.5x** | | |
|  | Y | U | V | Y | U | V |
| Class A | -0.54% | -0.27% | -0.37% |  |  |  |
| Class B | -0.94% | -0.51% | -0.60% | -0.58% | -0.10% | -0.13% |
| **Overall (Test vs Ref)** | -0.82% | -0.44% | -0.53% | -0.58% | -0.10% | -0.13% |
| **Overall (Test vs single layer)** | 11.46% | 13.14% | 12.77% | 9.63% | 10.18% | 9.57% |
| **EL only (Test vs Ref)** | -0.85% | -0.44% | -0.55% | -0.78% | -0.18% | -0.22% |
| Enc Time[%] | 162.0% | | | 153.5% | | |
| Dec Time[%] | 109.1% | | | 107.1% | | |
| Enc Mem[%] | 103.3% | | | 102.9% | | |
| BL Match | Matched | | | Matched | | |

# References

1. J. Chen, K. Rapaka, X. Li, V. Seregin, L. Guo, M. Karczewicz, G. Van der Auwera, J. Sole, X. Wang, C. J. Tu, Y. Chen, “Description of scalable video coding technology proposal by Qualcomm (configuration 1) JCTVC-K0035”, 11th Meeting of Joint Collaborative Team on Video Coding (JCT-VC) of ITU-T SG16 WP3 and ISO/IEC JTC1/SC29/WG11, Shanghai, China, 10-19 Oct., 2012
2. J. Chen, K. Rapaka, X. Li, V. Seregin, L. Guo, M. Karczewicz, G. Van der Auwera, J. Sole, X. Wang, C. J. Tu, Y. Chen, “Description of scalable video coding technology proposal by Qualcomm (configuration 2) JCTVC-K0036”, 11th Meeting of Joint Collaborative Team on Video Coding (JCT-VC) of ITU-T SG16 WP3 and ISO/IEC JTC1/SC29/WG11, Shanghai, China, 10-19 Oct., 2012.
3. K. Rapaka, J. Chen, X. Li, M. Karczewicz, "Non-TE3 : Simplification of Difference Intra Prediction In SHVC",JCTVC-L0294, Geneva, Switzerland, 14-23 Jan. 2013
4. [X. Li](mailto:lxiang@qti.qualcomm.com), [J. Boyce](mailto:jill@vidyo.com), [P. Onno](mailto:patrice.onno@crf.canon.fr), [Y. Ye](mailto:yan.ye@interdigital.com), “Common SHM test conditions and software reference configurations”, JCTVC-L1009, Geneva, Switzerland, 14–23 Jan. 2013

# Patent rights declaration(s)

**Qualcomm Incorporated may have current or pending patent rights relating to the technology described in this contribution and, conditioned on reciprocity, is prepared to grant licenses under reasonable and non-discriminatory terms as necessary for implementation of the resulting ITU-T Recommendation | ISO/IEC International Standard (per box 2 of the ITU-T/ITU-R/ISO/IEC patent statement and licensing declaration form).**