| Table 9‑43 – Assignment of ctxInc to syntax elements with context coded bins | | | | | | |
| --- | --- | --- | --- | --- | --- | --- |
| **Syntax element** | **binIdx** | | | | | |
| **0** | **1** | **2** | **3** | **4** | **>= 5** |
| … |  |  |  |  |  |  |
| palette\_share\_flag | bypass | na | na | na | na | na |
| palette\_predictor\_run | bypass | bypass | bypass | bypass | bypass | bypass |
| palette\_num\_signalled\_entries | bypass | bypass | bypass | bypass | bypass | bypass |
| palette\_entry | bypass | bypass | bypass | bypass | bypass | bypass |
| palette\_escape\_val\_present\_flag | bypass | na | na | na | na | na |
| cu\_qp\_delta\_palette\_abs | 0 | 1 | 1 | 1 | 1 | bypass |
| cu\_qp\_delta\_palette\_sign\_flag | bypass | na | na | na | na | na |
| cu\_chroma\_qp\_palette\_offset\_flag | 0 | na | na | na | na | na |
| cu\_chroma\_qp\_palette\_offset\_idx | 0 | 0 | 0 | 0 | 0 | na |
| palette\_transpose\_flag | 0, 1 (subclause 9.3.4.2.2) | na | na | na | na | na |
| … |  |  |  |  |  |  |