|  |  |
| --- | --- |
| **Joint Collaborative Team on 3D Video Coding Extension Development**  **of ITU-T SG 16 WP 3 and ISO/IEC JTC 1/SC 29/WG 11**  5th Meeting: Vienna, AT, 27 July – 2 Aug. 2013 | Document: JCT3V- E0198 |

|  |  |  |  |
| --- | --- | --- | --- |
| *Title:* | **CE 6.h: Crosscheck on CE results on sub-sampling for all SDC blocks (JCT3V-E0221)** | | |
| *Status:* | Input Document | | |
| *Purpose:* | Proposal | | |
| *Author(s) or Contact(s):* | Hongbin Liu ([hongbin.liu@lge.com](mailto:hongbin.liu@lge.com))  Junghak Nam ([junghak.nam@lge.com](mailto:junghak.nam@lge.com)) |  |  |
| *Source:* | LG Electronics | | |

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

# Abstract

This contribution reports a cross-check of JCT3V-E0221. Experiment results perfectly match with that provided in JCT3V-E0221.

# Results

Results for both CTC and AI are tested.

Table 1: performance comparison with HTM-7.0r1 (CTC)

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | video 0 | video 1 | video 2 | video PSNR / video bitrate | video PSNR / total bitrate | synth PSNR / total bitrate | enc time | dec time |
| Balloons | 0.00% | -0.07% | -0.09% | -0.03% | -0.03% | -0.07% | 76.0% | 103.0% |
| Kendo | 0.00% | 0.05% | -0.10% | 0.00% | 0.04% | 0.08% | 100.6% | 102.7% |
| Newspaper\_CC | 0.00% | -0.12% | -0.20% | -0.05% | -0.08% | -0.22% | 74.9% | 103.4% |
| GT\_Fly | 0.00% | 0.10% | -0.02% | 0.01% | -0.02% | -0.04% | 100.5% | 102.6% |
| Poznan\_Hall2 | 0.00% | 0.11% | 0.38% | 0.09% | 0.10% | 0.10% | 80.4% | 103.0% |
| Poznan\_Street | 0.00% | -0.10% | 0.11% | -0.01% | -0.02% | -0.02% | 84.1% | 103.0% |
| Undo\_Dancer | 0.00% | 0.07% | 0.28% | 0.05% | 0.03% | 0.08% | 100.4% | 102.3% |
| 1024x768 | 0.00% | -0.05% | -0.13% | -0.03% | -0.02% | -0.07% | 83.8% | 103.0% |
| 1920x1088 | 0.00% | 0.04% | 0.19% | 0.03% | 0.02% | 0.03% | 91.3% | 102.7% |
| **average** | **0.00%** | **0.00%** | **0.05%** | **0.01%** | **0.00%** | **-0.01%** | **88.1%** | **102.9%** |

Table 2: performance comparison with HTM-7.0r1 (AI)

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | video 0 | video 1 | video 2 | video PSNR / video bitrate | video PSNR / total bitrate | synth PSNR / total bitrate | enc time | dec time |
| Balloons | 0.00% | 0.00% | 0.00% | 0.00% | -0.02% | 0.02% | 99.9% | 102.3% |
| Kendo | 0.00% | 0.00% | 0.00% | 0.00% | -0.01% | -0.02% | 100.1% | 100.0% |
| Newspaper\_CC | 0.00% | 0.00% | 0.00% | 0.00% | -0.02% | 0.00% | 100.1% | 100.9% |
| GT\_Fly | 0.00% | 0.00% | 0.00% | 0.00% | -0.02% | 0.01% | 101.5% | 98.3% |
| Poznan\_Hall2 | 0.00% | 0.00% | 0.00% | 0.00% | -0.01% | -0.02% | 99.8% | 99.9% |
| Poznan\_Street | 0.00% | 0.00% | 0.00% | 0.00% | -0.01% | -0.01% | 102.9% | 99.1% |
| Undo\_Dancer | 0.00% | 0.00% | 0.00% | 0.00% | -0.01% | 0.01% | 99.9% | 98.2% |
| 1024x768 | 0.00% | 0.00% | 0.00% | 0.00% | -0.02% | 0.00% | 100.0% | 101.1% |
| 1920x1088 | 0.00% | 0.00% | 0.00% | 0.00% | -0.01% | 0.00% | 101.0% | 98.9% |
| **average** | **0.00%** | **0.00%** | **0.00%** | **0.00%** | **-0.01%** | **0.00%** | **100.6%** | **99.8%** |

# Conclusion

The result perfectly matches with JCT3V-E0221.