|  |  |
| --- | --- |
| **Joint Collaborative Team on 3D Video Coding Extension Development**  **of ITU-T SG 16 WP 3 and ISO/IEC JTC 1/SC 29/WG 11**  5th Meeting: Vienna, AT, 27 July – 2 Aug. 2013 | Document: JCT3V- E0238 |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| *Title:* | **3D-CE5.h related: Fast Intra Prediction Mode Selection for Intra Depth Map Coding** | | | |
| *Status:* | Input Document | | | |
| *Purpose:* | Proposal | | | |
| *Author(s) or Contact(s):* | Zhouye Gu1  Jianhua Zheng2  Nam Ling1  Philipp Zhang2 | Tel: +1-206-816-2367 Email: zgu@scu.edu  zhengjianhua@hisilicon.com | |  |
| *Source:* Santa Clara University1 and HiSilicon Technologies2 | | |  | |

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

# Abstract

This contribution proposes simplification of mode decision process on HEVC depth intra coding. In this contribution, it is proposed that for most the cases, the Depth Modelling Mode (DMM) and Region Boundary Chain mode[1] full-RD search could be skipped since the most CU is very flat or smooth and those modes are designed for depth CU with edge or sharp transition. Using the first mode in the full-RD search list and the block variance as indicators, we proposed a fast mode decision algorithm speedup the intra depth map encoding process. The test results on HTM7.0r1 platform report 26.5% encoding time saving with no bitrate loss for All-Intra test case. 2.35% encoding time saving and 10.4% decoding time saving is reported under CTC without any bitrate loss. The test results on the HM10-based platform HTM\_DEV\_0.3\_dev1 are consistent with the results on HTM7.0r1 platform.

# Introduction

In current 3D-HEVC design[1], DMMs and Region Boundary Chain mode are utilized together with the intra coding modes of HEVC for depth map intra coding. During the mode selection process, a full RD search list is created and several intra prediction modes are selected from all intra prediction modes for full-RD cost calculation. Then all the DMMs and Region Boundary Chain modes are also added to the full-RD search list. It is observed that after full-RD search, DMMs and Region Boundary Chain mode have comparatively lower probability to be selected as best mode. This is because most of the CUs in depth map are flat or smooth, while DMMs and Region Boundary Chain mode are designed for CU with edge or sharp transition thus are less efficient for smooth CU compression.

# Proposed Solution

Based on this observation, we propose a method to early terminate the DMMs and Region Boundary Chain mode full-RD cost calculation with the following two conditions:

## Mode Selection based on the first mode in full-RD cost calculation list

It is observed that when the first mode in full-RD cost calculation list is planar mode (uiRdModeList[0] == 0), the CU is very likely to be flat or smooth. Therefore, we will add all the DMMs and Region Boundary Chain mode to full-RD cost calculations if the first mode in full-RD cost calculation list is not planar mode (uiRdModeList[0] != 0).

## Mode Selection based on the CU Variance

Another observation is that the variance of CUs selecting DMMs and Region Boundary Chain mode as best mode is often higher than that of CUs selecting intra prediction modes as best mode. Therefore, we will also add all the DMMs and Region Boundary Chain mode to full-RD cost calculations if the variance of current CU is higher than a threshold (varThreshold in Eqn. (2)), which is defined as

threshold = max(((pcCU->getQP(0))>>3)-1,3); (1)

varThreshold = threshold\*threshold - 8; (2)

Combining condition 2.1 and 2.2, the additional condition we check before adding DMMs and Region Boundary Chain mode to full-RD cost calculations is:

(first mode in full-RD cost calculation list is not planar mode) || (CU variance >= varThreshold) (3)

Considering existing conditions, we summarize our fast intra depth map mode selection algorithm in Figure 1.



Figure 1. Flow chart of proposed fast mode selection algorithm for intra depth map coding

# Experimental Results

The proposed method is implemented on HTM7.0r1 software.

Table 1 shows the coding performance of 3-view case under common test condition for random access. No coding loss is observed and 10.4% deocoding time saving is achieved. Table 2 shows the coding performance of 3-view case for all intra case. No coding loss is observed and 26.5% encoding time saving is achieved.

Table 1. BD rate results for 3-view case under CTC, Random Access



Table 2. BD rate results for 3-view case under CTC, ALL Intra



Table 3. Full RD Search Cycle Reduction

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
|  | QP = 25\_34 | QP = 30\_39 | QP = 35\_42 | QP = 40\_45 | Average Saving  of each Sequence |
| GTfly | 31.09% | 26.19% | 27.76% | 29.46% | **28.63%** |
| Kendo | 17.11% | 16.46% | 18.86% | 23.89% | **19.08%** |
| Newspaper | 27.97% | 24.55% | 23.38% | 29.97% | **26.46%** |
| PoznanHall | 28.08% | 24.86% | 28.88% | 31.59% | **28.35%** |
| Poznanstreet | 26.79% | 27.19% | 24.10% | 27.29% | **26.34%** |
| Balloon | 19.15% | 19.97% | 22.04% | 27.40% | **22.14%** |
| UndoDancer | 29.88% | 29.25% | 28.12% | 28.68% | **28.98%** |
| **Average** | **25.72%** | **24.07%** | **24.74%** | **28.33** % | **25.71%** |

Beside run time saving, we further provide the Full-RD search cycle reduction (percentage of reduction of candidate modes for full-RD search) in Table 3. As observed, more than 25% Full RD search cycles are saved based on proposed algorithm.

To evaluate the consistency of the proposed method over the new HM10 based HTM software, the method is also implemented on HTM\_DEV\_0.3\_dev1, and the coding performance under HTM\_DEV\_0.3\_dev1 is summarized in Table 4 and Table 5. Considerable encoding time saving is still achieved without any bitrate loss.

Table 4. BD rate results for 3-view case under CTC, Random Access (Version: HTM\_DEV\_0.3\_dev1)



Table 5. BD rate results for 3-view case under CTC, ALL Intra (Version: HTM\_DEV\_0.3\_dev1)



# Conclusion

Fast mode selection algorithms of intra depth coding for 3D-HEVC is proposed. It is reported that for all intra test, the proposed algorithm achieves 26.5% encoding time saving without any bitrate loss. For random access case, 10.4% decoding time saving is achieved without any bitrate loss. It is suggested to inlcude the fast intra depth map mode selection method in the new HTM software and be enable under CTC.

# References

[1] Jin Heo, Eunyong Son, Sehoon Yea, “Region boundary chain coding for depth-map”, JCT3V-A0070, 1st Meeting: Stockholm, SE, 16–20 July 2012.

# Patent rights declaration(s)

**HiSilicon Technologies, Santa Clara University and Huawei Technologies may have current or pending patent rights relating to the technology described in this contribution and, conditioned on reciprocity, is prepared to grant licenses under reasonable and non-discriminatory terms as necessary for implementation of the resulting ITU-T Recommendation | ISO/IEC International Standard (per box 2 of the ITU-T/ITU-R/ISO/IEC patent statement and licensing declaration form).**