|  |  |
| --- | --- |
| **Joint Collaborative Team on Video Coding (JCT-VC)**  **of ITU-T SG 16 WP 3 and ISO/IEC JTC 1/SC 29/WG 11**  10th Meeting: Stockholm, SE, 11–20 July 2012 | Document: JCTVC-J0457 |

|  |  |  |  |
| --- | --- | --- | --- |
| *Title:* | **Mental cross-check of JCTVC-J0072** | | |
| *Status:* | Input Document to JCT-VC | | |
| *Purpose:* | Information | | |
| *Author(s) or Contact(s):* | Ye-Kui Wang  5775 Morehouse Drive, San Diego, CA 92121-1714 USA | Tel: Email: | 1-858-651-8345 [yekuiw@qualcomm.com](mailto:yekuiw@qualcomm.com) |
| *Source:* | Qualcomm Incorporated | | |

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

# Abstract

This document provides a mental cross-check for JCTVC-J0072.

It is claimed that the authors of this document basically understand what is being proposed in JCTVC-J0072. The authors of this document would like to summarize the proposal in JCTVC-J0072 as follows.

JCTVC-J0072 proposes a mechanism to enable detection of the loss of an updated APS, for which the aps\_id value has been used previously by another APS NAL unit. The mechanism imposes a constraint on assignment of aps\_id values and thus limits how APSs can be updated. Normative changes being proposed include addition of two syntax elements to the SPS syntax and a change to the APS activation process.

# Patent rights declaration(s)

**Qualcomm Incorporated does not have current or pending patent rights relating to the technology described in this contribution.**