Append to “2.4 Additional references”:

*“* – ISO/IEC 23001-11 (in force), *Information Technology — MPEG Systems technologies — Part 11: Energy-efficient media consumption (green metadata).”*

In Table D.2.1, after “decoded\_picture\_hash( payloadSize )”, insert:

|  |  |
| --- | --- |
| else if( payloadType == 133 ) |  |
| green\_metadata( payloadSize ) /\* specified in ISO/IEC 23001-11 \*/ |  |

*Renumber “****D.2.35******Reserved SEI message syntax”*** *to “****D.2.36******Reserved SEI message syntax”****.*

*Renumber “****D.3.35******Reserved SEI message semantics”*** *to “****D.3.36******Reserved SEI message semantics”****.*

*Add the following after D.2.34:*

**D.2.35 Green metadata SEI message syntax:**

The syntax for this SEI message is specified in ISO/IEC 23001-11 (Green metadata). Green metadata facilitates reduced power consumption in decoders, encoders, displays and in media selection.

*Add the following after D.3.34:*

**D.3.35 Green metadata SEI message semantics**

The semantics for this SEI message are specified in ISO/IEC 23001-11 (Green metadata). Green metadata facilitates reduced power consumption in decoders, encoders, displays and in media selection.