|  |  |
| --- | --- |
| **Joint Collaborative Team on 3D Video Coding Extension Development**  **of ITU-T SG 16 WP 3 and ISO/IEC JTC 1/SC 29/WG 11**  4th Meeting: Incheon, KR, 20–26 Apr. 2013 | Document: JCT3V- Dxxxx |

|  |  |  |  |
| --- | --- | --- | --- |
| *Title:* | **CE6.h related : Removal of DC from SDC Mode** | | |
| *Status:* | Input Document | | |
| *Purpose:* | Proposal | | |
| *Author(s) or Contact(s):* |  |  |  |
| *Source:* | LG Electronics | | |

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Spec change:

~~Table H‑4 – Interpretation of sdc\_pred\_mode~~

|  |  |
| --- | --- |
| **~~sdc\_pred\_mode~~** | ~~Associated Intra Prediction Mode~~ |
| ~~0~~ | ~~Intra\_DC~~ |
| ~~1~~ | ~~Intra\_DepthPartition( 35 )~~ |
| ~~2~~ | ~~Intra\_Planar~~ |

Table H‑ – Interpretation of sdc\_pred\_mode

|  |  |
| --- | --- |
| **sdc\_pred\_mode** | Associated Intra Prediction Mode |
| 1 | Intra\_DepthPartition( 35 ) |
| 0 | Intra\_Planar |