|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Syntax structure** | **Syntax element** | **ctxTable** | **initType** | | |
| **0** | **1** | **2** |
| cu\_extension( )  intra\_mode\_ext( ) | depth\_intra\_mode\_flag |  | 0 | 1 | 2 |
| ~~wedge\_full\_tab\_idx~~ |  | ~~0~~ | ~~1~~ | ~~2~~ |

Table I 12 – Association of ctxIdx and syntax elements for each initializationType in the initialization process

~~Table ‑13 – Values of initValue for wedge\_full\_tab\_idx ctxIdx~~

|  |  |  |  |
| --- | --- | --- | --- |
| **~~Initialization variable~~** | **~~ctxIdx of wedge\_full\_tab\_idx~~** | | |
| **~~0~~** | **~~1~~** | **~~2~~** |
| **~~initValue~~** | ~~154~~ | ~~154~~ | ~~154~~ |

Table ‑23 –Assignment of ctxInc to syntax elements with context coded bins

| **Syntax element** | **binIdx** | | | | | |
| --- | --- | --- | --- | --- | --- | --- |
| **0** | **1** | **2** | **3** | **4** | **>=5** |
| wedge\_full\_tab\_idx | ~~0~~ bypass | ~~0~~ bypass | ~~0~~ bypass | ~~0~~ bypass | ~~0~~ bypass | ~~0~~ bypass |